Maintain an M60 Machine Gun Reviews
Summary – Disassemble the M60 Machine Gun
21 of 44
&pageText=You should now be comfortable with the process
for disassembling the M60 machine gun. To disassemble the M60, you must remove:& &bulletText1=Stock group& &bulletText2=Buffer, operating rod, and bolt assembly group& &bulletText3=Trigger mechanism group& &bulletText4=Cover, feed tray, and hanger group& &bulletText5=Barrel group& &bulletText6=Forearm assembly& &bulletTime1=8300& &bulletTime2=10600& &bulletTime3=13300& &bulletTime4=15300& &bulletTime5=17300& &bulletTime6=18900& &numBullets=6& &timedText=true& &audioXpos=375& &audioYpos=20&