Maintain an M60 Machine Gun Reviews
Disassemble the M60 Machine Gun
12 of 44
&pageText=After you have ensured the M60 is clear, it is safe to disassemble the machine gun in order to clean, inspect, and lubricate the parts. To disassemble the M60, you must remove:& &label1=Stock group& &label2=Buffer, operating rod, and bolt assembly group& &label3=Trigger mechanism group& &label4=Cover, feed tray, and hanger group& &label5=Barrel group& &label6=Forearm assembly& &instructionText=Click on the Next button to continue.& &sub1=1& &page1=0010& &sub2=2& &page2=0010& &sub3=3& &page3=0010& &sub4=4& &page4=0010& &sub5=5& &page5=0010& &sub6=6& &page6=0010&