Maintain an M60 Machine Gun Reviews
Quick Review 5
29 of 44
&questionText=Determine the correct answer to the question and indicate your answer by clicking the letter next to your choice.
Which of the following options correctly describes how to lubricate the exterior metal surfaces of the M60 machine gun?& &lure1=Using a swab dampened with CLP& &lure2=Using a receiver brush dampened with CLP& &lure3=Using a rag dampened with CLP& &lure4=Using a clean, dry wiping rag& &correctResponse=3& &attempts=2& &correctFeedback=Nice work. To properly lubricate the exterior metal surfaces of the M60 machine gun, you should use a rag dampened with CLP.& &correctFeedback2=Nice work. To properly lubricate the exterior metal surfaces of the M60 machine gun, you should use a rag dampened with CLP.& &incorrectFeedback1=That is incorrect. Visualize lubricating the outside of the M60 receiver group and try again. Remember, this does not include any plastic or rubber-coated parts.& &failedFeedback=You still have not mastered the steps in lubricating the M60 machine gun.& &link=a404p0180.html& &mediaStyle=swf&