Maintain an M249 Machine Gun Reviews
Handguard Group
46 of 54
&pageText=The fifth step in the assembly of the M249 machine gun involves placing the handguard group back on the receiver group, by:& &bulletText1=Placing it on the receiver from the bottom and pushing it to the rear until it stops& &bulletText2=Using the guide rod, push the handguard retaining pin to the right, which will lock the handguard into position, then push the handguard down to be sure that it is locked in place& &bulletTime1=8100& &bulletTime2=15900& &numBullets=2& &timedText=true& &audioBorder=false& &enableBtns=audio& &audioXpos=350& &audioYpos=100&