Maintain an M249 Machine Gun Reviews
Gas Cylinder Group
15 of 54
&pageText=The sixth step in the disassembly of the M249 machine gun involves the disassembly of the gas cylinder group from the receiver group by grasping the gas cylinder at the top of the bipod legs and rotating it to the left or right to release the locking spring, and then pull it away from the receiver group.& &mediaStyle=swf& &textPosition=top& &imageBorder=true&