Maintain an M249 Machine Gun Reviews
Disassemble the M249 Machine Gun
9 of 54
&pageText=The disassembly of the machine gun is an eight-step process. During disassembly, each part is laid out on a flat surface. This will aid in reassembling the weapon in reverse order and avoids the possible loss of parts. To disassemble the machine gun, complete the disassembly procedures for each of the eight major groups:& &label1=Operating rod group& &label2=Barrel group& &label3=Handguard group& &label4=Buttstock and buffer assembly group& &label5=Trigger mechanism group& &label6=Gas cylinder group& &label7=Bipod group& &label8=Receiver group& &sub1=1& &page1=0010& &sub2=2& &page2=0010& &sub3=3& &page3=0010& &sub4=4& &page4=0010& &sub5=5& &page5=0010& &sub6=6& &page6=0010& &sub7=7& &page7=0010& &sub8=8& &page8=0010& &enableBtns=audio& &instructionText=Click on the Next button to continue.&