Maintain an M249 Machine Gun Reviews
Introduction to Assemble the Machine Gun
40 of 54
&pageText=The sixth performance measure in maintaining the machine gun is the reassembly of the weapon. The M249 machine gun is reassembled in reverse order of the disassembly process. To assemble the machine gun, you must correctly reassemble each of the eight major groups:& &bullet1=• Receiver group& &bullet2=• Bipod group& &bullet3=• Gas cylinder group& &bullet4=• Trigger mechanism group& &bullet5=• Buttstock and buffer assembly group& &bullet6=• Handguard group& &bullet7=• Barrel group& &bullet8=• Operating rod group&