Lead a Convoy Serial/March Unit Reviews
Quick Review 11
39 of 48
&pageText=Situation: You continue to prepare for your tactical convoy with two march units of 20 vehicles each. You instruct all convoy drivers and assistants to perform before operation PMCS on their vehicles using the appropriate 10-level manuals. You and the other leaders of your convoy supervise the PMCS. Click the space next to the items that must be checked, repaired, filled or adjusted during the before operation PMCS.& &lure1=Air hose couplings& &lure2=Protective sandbags& &lure3=Oil and lubrication levels& &lure4=Cooling systems& &lure5=Brakes& &lure6=Cargo containers& &lure7=Tires& &feedback=That is correct. The air hose couplings, oil and lubrication levels, cooling systems, brakes, and tires must be checked, repaired, filled or adjusted during the before operation PMCS.
Click the Next button to continue.& &negFeedback1=That is incorrect. Carefully review the items that must be checked, repaired, filled or adjusted during the before operation PMCS. Try the Quick Review again.& &negFeedback2=That is also incorrect. The air hose couplings, oil and lubrication levels, cooling systems, brakes, and tires must be checked, repaired, filled or adjusted during the before operation PMCS.& &link=a399p0200&