RAD Studio |  |

Table Of CodeGear C++ Register Pseudovariables

This table lists all pseudovariables.

_AH | _CL | _EAX | _ESP
_AL | _CS | _EBP | _FLAGS
_AX | _CX | _EBX | _FS
_BH | _DH | _ECX | _GS
_BL | _DI | _EDI | _SI
_BP | _DL | _EDX | _SP
_BX | _DS | _ES | _SS
_CH | _DX | _ESI |

All but the _FLAGS and _EFLAGS register pseudovariables are associated with the general purpose, segment, address, and special purpose registers.

Use register pseudovariables anywhere that you can use an integer variable to directly access the corresponding 80x86 register.

The flags registers contain information about the state of the 80x86 and the results of recent instructions.

Copyright(C) 2009 Embarcadero Technologies, Inc. All Rights Reserved.
What do you think about this topic? Send feedback!